As there are quite a lot of packets in the capture, check statistics first in Wireshark:

Statistics->IPv4 Statistics:

A screenshot of a computer

Description automatically generated

Let’s check the private IP communication first and follow the DNS stream:

A screen shot of a computer

Description automatically generated

Copy the 2 DNS hostname combined together and decoded using base64:

A screenshot of a computer

Description automatically generated

Flag: MOCSCTF{y0u\_d15c0v3r\_dn5\_3xf11tr@t10n!}